{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A8"]
[]
[]
[]
[]
["","","","","","RXM50A5V1B8"]
["Wymiary","Jednostka","","Wysokość","mm","610"]
["","","","Szerokość","mm","923"]
["","","","Głębokość","mm","367"]
["Ciężar","Jednostka","","","kg","40"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","600"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (1), 46 (1)"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-21 (1), -15 (1)"]
["","","","Maks.","°CWB","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","48"]
["","Grzanie","","Nom.","dBA","49"]
["Czynnik chłodniczy","Typ","","","","R-32"]
["","Ilość","","","kg","0.95"]
["","Ilość","","","tCO2Eq","0.65"]
["","GWP","","","","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","20"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Złącze spustowe","","","","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","1"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","1"]
["","Etykieta klasy energetycznej LOT10","","","","1"]
["","Nasadka spustowa","","","","3"]
["Zakres efektywności energetycznej","","","","","A+++ ~ D"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]
["Uwagi","","","","","(1) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(2) - Dane elektryczne, patrz oddzielny rysunek"]
["","","","","","(3) - Zawiera fluorowane gazy cieplarniane"]