{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M9"]
[]
[]
[]
[]
["","","","","","RXM20M3V1B9","RXM25M3V1B9","RXM35M3V1B9","RXM42M3V1B9 (Archived)","RXM50M3V1B9 (Archived)","RXM60M3V1B9 (Archived)"]
["Wymiary","Jednostka","","Wysokość","mm","550","550","550","735","735","735"]
["","","","Szerokość","mm","765","765","765","825","825","825"]
["","","","Głębokość","mm","285","285","285","300","300","300"]
["Ciężar","Jednostka","","","kg","32","32","32","47","47","47"]
["Sprężarka","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","46","46","49","48","48","48"]
["","Grzanie","","Nom.","dBA","47","47","49","48","49","49"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Ilość","","","kg","0.76","0.76","0.76","1.30","1.40","1.45"]
["","Ilość","","","tCO2Eq","0.52","0.52","0.52","0.88","0.95","0.98"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20.0","20.0","20.0","30","30","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15.0","15.0","15.0","20","20","20"]
["Standardowe akcesoria","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~","1~","1~","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Sprężarka","Typ","","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]