{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","49","","","52"]
["","","","Niski","dBA","46","","","49"]
["","Chłodzenie","","Niski","dBA","46","","","49"]
["","","","Wysoki","dBA","49","","","52"]
["Standardowe akcesoria","Gniazdo spustowe","","","","1","","","1"]
["","Instrukcja instalacji","","","","1","","","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Ilość","","","kg","1.5","","","2.3"]
["","Typ","","","","R-410A","","","R-410A"]
["Piping connections","Różnica poziomów","IU - OU","Maks.","m","20","","","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","","","65"]
["Sprężarka","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","825","","","900"]
["","","","Głębokość","mm","300","","","320"]
["","","","Wysokość","mm","735","","","770"]
["Ciężar","Jednostka","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Częstotliwość","","","Hz","50","","","50"]
["","Napięcie","","","V","220-240","","","220-240"]
["Uwagi","","","","","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","(1) - 220 V","","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","(1) - 220 V"]
["","","","","","(2) - Zawiera fluorowane gazy cieplarniane","(2) - 230 V","","(2) - Zawiera fluorowane gazy cieplarniane","(2) - 230 V"]
["Wymiary","Jednostka","","Wysokość","mm","","735","735","","770","770"]
["","","","Szerokość","mm","","825","825","","900","900"]
["","","","Głębokość","mm","","300","300","","320","320"]
["Ciężar","Jednostka","","","kg","","48","48","","71","71"]
["Sprężarka","Type","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Maks.","°CDB","","46","46","","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","-15","-15","","-15","-15"]
["","","","Maks.","°CWB","","18","20","","18","20"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","49","49","","52","52"]
["","","","Niski","dBA","","46","46","","49","49"]
["","Grzanie","","Wysoki","dBA","","49","49","","52","52"]
["","","","Niski","dBA","","46","46","","49","49"]
["Czynnik chłodniczy","Typ","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Ilość","","","kg","","1.5","1.5","","2.3","2.3"]
["","Ilość","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","30","30","","30","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","20","20","","20","20"]
["Standardowe akcesoria","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Zasilanie energią elektryczną","liczba faz","","","","","1~","1~","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50","50","","50","50"]
["","Napięcie","","","V","","220-240","220-240","","220-240","220-240"]
["Uwagi","","","","","","(3) - 240 V","","","(3) - 240 V"]
["Standardowe akcesoria","Drain socket","","","","","","1","","","1"]