{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","46.0"]
["","","Ogrzewanie","Bardzo niska","m³/min","46.0"]
["","","","Bardzo niska","cfm","1624"]
["","","Ogrzewanie","Bardzo niska","cfm","1624"]
["Wymiary","Jednostka","","Wysokość","mm","770"]
["","","","Szerokość","mm","900"]
["","","","Głębokość","mm","320"]
["Ciężar","Jednostka","","","kg","71"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","730"]
["","","Ogrzewanie","Bardzo niska","obr/min_","730"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","52"]
["","Grzanie","","Wysoki","dBA","52"]
["Czynnik chłodniczy","Typ","","","","R-410A"]
["","Ilość","","","kg","2.3"]
["","Ilość","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","20"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]
["Uwagi","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]