{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Poziom ciś. akust.","Grzanie","","Wysoki","dBA","47","","47","","48","48","48"]
["","Chłodzenie","","Wysoki","dBA","46","","46","","48","48","48"]
["Standardowe akcesoria","Złącze (spustowe)","","","","1","","1"]
["","Instrukcja instalacji","","","","1","","1","","1","1","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Ilość","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Typ","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Fan motor","Prędkość obrot.","Chłodzenie","Bardzo niska","obr/min","780","","780","","780","790","670"]
["","","Grzanie","Bardzo niska","obr/min","740","","740","","740","780","670"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - OU","Maks.","m","15","","15","","15","15","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Compressor","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","","Sprężarka typu \"swing\" uszczelniona hermetycznie","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","765","","765","","765","765","825"]
["","","","Głębokość","mm","285","","285","","285","285","300"]
["","","","Wysokość","mm","550","","550","","550","550","735"]
["Ciężar","Jednostka","","","kg","34","","34","","34","39","47"]
["Wentylator","Natężenie przepł. pow.","Grzanie","Bardzo niska","cfm","","","","","904","960","1,522"]
["","","Chłodzenie","Bardzo niska","cfm","","","","","1,063","1,080","1,727"]
["Power supply","liczba faz","","","","1~","","1~","","1~","1~","1~"]
["","Częstotliwość","","","Hz","50","","50","","50","50","50"]
["","Napięcie","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","","(4) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza","","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(5) - Zawiera fluorowane gazy cieplarniane","","(5) - Zawiera fluorowane gazy cieplarniane"]
["Wymiary","Jednostka","","Wysokość","mm","","550","","550"]
["","","","Szerokość","mm","","765","","765"]
["","","","Głębokość","mm","","285","","285"]
["Ciężar","Jednostka","","","kg","","34","","34"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min","","780","","780"]
["","","Ogrzewanie","Bardzo niska","obr/min","","740","","740"]
["Compressor","Type","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","-10","","-10"]
["","","","Maks.","°CDB","","46","","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","-15","","-15"]
["","","","Maks.","°CWB","","18","","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","46","","46"]
["","Grzanie","","Wysoki","dBA","","47","","47"]
["Czynnik chłodniczy","Typ","","","","","R-410A","","R-410A"]
["","Ilość","","","kg","","1.0","","1.0"]
["","Ilość","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","20","","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","15","","15"]
["Standardowe akcesoria","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","","1~","","1~"]
["Zasilanie","Częstotliwość","","","Hz","","50","","50"]
["","Napięcie","","","V","","220-240","","220-240"]
["Standardowe akcesoria","Korek spustowy","","","","","","","","1","1","1"]