{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","47","47","48","48"]
["","Chłodzenie","","Wysoki","dBA","46","46","48","48"]
["Standardowe akcesoria","Nasadka spustowa","","","","1","1","","1"]
["","Instrukcja instalacji","","","","1","1","1","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","1","1","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","1","1","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","1.0","1.20","1.3"]
["","Typ","","","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Prędkość","Chłodzenie","Bardzo niska","obr/min_","780","780","780","790"]
["","","Grzanie","Bardzo niska","obr/min_","740","740","740","780"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Maks.","°CDB","46","46","46","46"]
["","","","Min.","°CDB","-10","-10","-10","-10"]
["","Heating","Temp. otoczenia","Maks.","°CWB","18","18","18","18"]
["","","","Min.","°CWB","-15","-15","-15","-15"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - OU","Maks.","m","","","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","","0,020 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Wymiary","Jednostka","","Szerokość","mm","765","765","765","765"]
["","","","Głębokość","mm","285","285","285","285"]
["","","","Wysokość","mm","550","550","550","550"]
["Compressor","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Ciężar","Jednostka","","","kg","34","34","34","39"]
["Wentylator","Przepływ powietrza","Grzanie","Bardzo niska","cfm","904","904","904","960"]
["","","","Bardzo niska","m³/min","25.6","25.6","25.6","27.2"]
["","","Chłodzenie","Bardzo niska","m³/min","30.1","30.1","30.1","30.6"]
["","","","Bardzo niska","cfm","1,063","1,063","1,063","1,080"]
["Power supply","liczba faz","","","","1~","1~","1~","1~"]
["","Częstotliwość","","","Hz","50","50","50","50"]
["","Napięcie","","","V","220-240","220-240","220-240","220-240"]
["Uwagi","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane","(4) - Zawiera fluorowane gazy cieplarniane"]
["Standardowe akcesoria","Korek spustowy","","","","","","1"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","","","","","48.9","45.0"]
["","","Ogrzewanie","Bardzo niska","m³/min","","","","","43.1","46.3"]
["","","","Bardzo niska","cfm","","","","","1727","1589"]
["","","Ogrzewanie","Bardzo niska","cfm","","","","","1522","1635"]
["Wymiary","Jednostka","","Wysokość","mm","","","","","735","735"]
["","","","Szerokość","mm","","","","","825","825"]
["","","","Głębokość","mm","","","","","300","300"]
["Ciężar","Jednostka","","","kg","","","","","47","48"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","","","","","670"]
["","","Ogrzewanie","Bardzo niska","obr/min_","","","","","670"]
["Sprężarka","Typ","","","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","","","","-10","-10"]
["","","","Maks.","°CDB","","","","","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","","","","-15","-15"]
["","","","Maks.","°CWB","","","","","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","","","","","48","49"]
["","","","Niski","dBA","","","","","44","46"]
["","Grzanie","","Wysoki","dBA","","","","","48","49"]
["","","","Niski","dBA","","","","","45","46"]
["Czynnik chłodniczy","Typ","","","","","","","","R-410A","R-410A"]
["","Ilość","","","kg","","","","","1.7","1.5"]
["","Ilość","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","","","","30","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","","","","0,020 (dla długości instalacji rurowej przekraczającej 10 m)","0,020 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","","","","","20.0","20"]
["Standardowe akcesoria","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Zasilanie energią elektryczną","liczba faz","","","","","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","","","","","50","50"]
["","Napięcie","","","V","","","","","220-230-240","220-230-240"]
["Uwagi","","","","","","","","","","(1) - 230 V"]