{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Poziom ciśnienia akustycznego","Grzanie","","Wysoki","dBA","","","48"]
["","Chłodzenie","","Wysoki","dBA","","","48"]
["Standardowe akcesoria","Instrukcja instalacji","","","","","","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","","","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","","","1"]
["","Korek spustowy (tylko modele z pompą ciepła)","","","","","","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Dopełnienie","","","kg","","","1.2"]
["","Typ","","","","","","R-410A"]
["Fan motor","Prędkość","Chłodzenie","Bardzo niska","obr/min","","","780"]
["","","Ogrzewanie","Bardzo niska","obr/min","","","740"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Maks.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Ogrzewanie","Temp. otoczenia","Maks.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Połączenia instalacji rurowej","Różnica poziomów","IU - OU","Maks.","m","","","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","","","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Wymiary","Jednostka","","Szerokość","mm","","","765"]
["","","","Głębokość","mm","","","285"]
["","","","Wysokość","mm","","","550"]
["Sprężarka","Typ","","","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Ciężar","Jednostka","","","kg","","","34"]
["Wentylator","Natężenie przepływu powietrza","Ogrzewanie","Bardzo niska","cfm","","","904"]
["","","","Bardzo niska","m³/min","","","25.6"]
["","","Chłodzenie","Bardzo niska","m³/min","","","30.1"]
["","","","Bardzo niska","cfm","","","1,063"]
["Power supply","liczba faz","","","","","","1~"]
["","Częstotliwość","","","Hz","","","50"]
["","Napięcie","","","V","","","220-240"]
["Uwagi","","","","","","","(1) - SL: poziom cichego wentylatora ustawienia szybkości przepływu powietrza"]
["Wentylator","Natężenie przepływu powietrza","Chłodzenie","Bardzo niska","m³/min","30.1","30.1"]
["","","Ogrzewanie","Bardzo niska","m³/min","25.6","25.6"]
["","","","Bardzo niska","cfm","1063","1063"]
["","","Ogrzewanie","Bardzo niska","cfm","904","904"]
["Wymiary","Jednostka","","Wysokość","mm","550","550"]
["","","","Szerokość","mm","765","765"]
["","","","Głębokość","mm","285","285"]
["Ciężar","Jednostka","","","kg","34","34"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min","780","780"]
["","","Ogrzewanie","Bardzo niska","obr/min","740","740"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15","-15"]
["","","","Maks.","°CWB","18","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","46","46"]
["","Grzanie","","Wysoki","dBA","47","47"]
["Czynnik chłodniczy","Typ","","","","R-410A","R-410A"]
["","Ilość","","","kg","1.0","1.0"]
["","Ilość","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15","15"]
["Standardowe akcesoria","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~","1~"]
["Zasilanie","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Standardowe akcesoria","Drain plug (only heat pump models)","","","","","1"]