{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-B"]
[]
[]
[]
[]
["","","","","","RXTA30B2V1B"]
["Wymiary","Jednostka","","Wysokość","mm","551"]
["","","","Szerokość","mm","763"]
["","","","Głębokość","mm","312"]
["Ciężar","Jednostka","","","kg","38"]
["Silnik wentylatora","Prędkość","Chłodzenie","Bardzo niska","obr/min_","450"]
["","","Ogrzewanie","Bardzo niska","obr/min_","360"]
["Sprężarka","Typ","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-25"]
["","","","Maks.","°CWB","18"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","48"]
["","Grzanie","","Nom.","dBA","49"]
["Czynnik chłodniczy","Typ","","","","R-32"]
["","Ilość","","","kg","1.1"]
["","Ilość","","","tCO2Eq","0.74"]
["","GWP","","","","675"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","20"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["","Różnica poziomów","IU - OU","Maks.","m","15"]
["Standardowe akcesoria","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Zasilanie energią elektryczną","liczba faz","","","","1~"]
["Zasilanie","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","220-240"]