{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N8"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B8","RXTP35N2V1B8"]
["Poziom ciśnienia akustycznego","Grzanie","","Nom.","dBA","49","49"]
["","Chłodzenie","","Nom.","dBA","48","48"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1"]
["","Etykieta z informacją o ładunku czynnika chłodniczego","","","","1","1"]
["","Wielojęzyczna etykieta z informacją o fluorowanych gazach cieplarnianych","","","","1","1"]
["Czynnik chłodniczy","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Ilość","","","kg","1.1","1.1"]
["","Typ","","","","R-32","R-32"]
["Fan motor","Prędkość obrot.","Chłodzenie","Bardzo niska","obr/min","450","450"]
["","","Grzanie","Bardzo niska","obr/min","360","360"]
["Piping connections","Różnica poziomów","IU - OU","Maks.","m","15","15"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","0,02 (dla długości instalacji rurowej przekraczającej 10 m)","0,02 (dla długości instalacji rurowej przekraczającej 10 m)"]
["Sprężarka","Type","","","","Sprężarka typu \"swing\" uszczelniona hermetycznie","Sprężarka typu \"swing\" uszczelniona hermetycznie"]
["Wymiary","Jednostka","","Szerokość","mm","763","763"]
["","","","Głębokość","mm","312","312"]
["","","","Wysokość","mm","551","551"]
["Ciężar","Jednostka","","","kg","38","38"]
["Power supply","Phase","","","","1~","1~"]
["","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","220-240","220-240"]
["Uwagi","","","","","(1) - Zawiera fluorowane gazy cieplarniane","(1) - Zawiera fluorowane gazy cieplarniane"]
["","","","","","(2) - Patrz oddzielny rysunek zakresu pracy","(2) - Patrz oddzielny rysunek zakresu pracy"]
["","","","","","(3) - Dane elektryczne, patrz oddzielny rysunek","(3) - Dane elektryczne, patrz oddzielny rysunek"]