{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Wymiary","Jednostka","","Wysokość","mm","870","870"]
["","","","Szerokość","mm","1,100","1,100"]
["","","","Głębokość","mm","460","460"]
["Ciężar","Jednostka","","","kg","117","117"]
["Compressor","Type","","","","Sprężarka spiralna uszczelniona hermetycznie","Sprężarka spiralna uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-20","-20"]
["","","","Maks.","°CDB","46","46"]
["","Heating","Temp. otoczenia","Min.","°CWB","-20","-20"]
["","","","Maks.","°CWB","15","15"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","73","76"]
["","Ogrzewanie","","","dBA","76 (1)","79 (1)"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Nom.","dBA","53","57"]
["","Grzanie","","Nom.","dBA","60","63"]
["Czynnik chłodniczy","Typ","","","","R-32","R-32"]
["","Ilość","","","kg","5","5"]
["","GWP","","","","675","675"]
["Piping connections","Ciecz","","Śr. zewn.","mm","9.52","9.52"]
["","Gaz","","Śr. zewn.","mm","22.2","22.2"]
["","Długość instalacji rurowej","Maks.","OU - IU","m","100","100"]
["","","System","Bez obciążenia","m","30","30"]
["","Dodatkowy ładunek czynnika chłodniczego","","","kg/m","Patrz instrukcja instalacji","Patrz instrukcja instalacji"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1","1"]
["","Ogólne zalecenia dotyczące bezpieczeństwa","","","","1","1"]
["","Wiązania","","","","2","2"]
["","Odlepiana etykieta o gazach fluorowanych","","","","1","1"]
["","Łączniki rurowe","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Częstotliwość","","","Hz","50","50"]
["","Napięcie","","","V","380-415","380-415"]
["Prąd - 50 Hz","Maksymalne amperaże bezpiecznika (MFA)","","","A","20","20"]
["Uwagi","","","","","(1) - Zgodnie z ENER Dział 21","(1) - Zgodnie z ENER Dział 21"]