{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Wymiary","Jednostka","","Wysokość","mm","1,680"]
["","","","Szerokość","mm","930"]
["","","","Głębokość","mm","765"]
["Ciężar","Jednostka","","","kg","183.0"]
["Sprężarka","Type","","","","Sprężarka spiralna uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","-5.0"]
["","","","Maks.","°CDB","46.0"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","-15.0"]
["","","","Maks.","°CWB","15.0"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","78.0"]
["","Ogrzewanie","","","dBA","78.0"]
["Czynnik chłodniczy","Typ","","","","R-410A"]
["","Ilość","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Piping connections","Ciecz","","Śr. zewn.","mm","9.52"]
["","Gaz","","Śr. zewn.","mm","22.2"]
["","Długość instalacji rurowej","Maks.","OU - IU","m","100"]
["","","System","Bez obciążenia","m","30"]
["Standardowe akcesoria","Instrukcja instalacji","","","","1"]
["","Łączniki rurowe","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Częstotliwość","","","Hz","50"]
["","Napięcie","","","V","380-415"]
["Prąd - 50 Hz","Maksymalne amperaże bezpiecznika (MFA)","","","A","25"]
["Uwagi","","","","","(1) - Zasilanie do jednostki wewnętrznej FDQ jest oddzielne"]
["","","","","","(2) - Dane elektryczne, patrz oddzielne rysunki"]
["Wymiary","Jednostka","","Wysokość","mm","","1680"]
["","","","Szerokość","mm","","930"]
["","","","Głębokość","mm","","765"]
["Ciężar","Jednostka","","","kg","","184.0"]
["Sprężarka","Typ","","","","","Sprężarka spiralna uszczelniona hermetycznie"]
["Zakres pracy","Chłodzenie","Temp. otoczenia","Min.","°CDB","","-5.0"]
["","","","Maks.","°CDB","","46.0"]
["","Grzanie","Temp. otoczenia","Min.","°CWB","","-15.0"]
["","","","Maks.","°CWB","","15.0"]
["Poziom mocy akustycznej","Chłodzenie","","","dBA","","78.0"]
["","Ogrzewanie","","","dBA","","78.0"]
["Czynnik chłodniczy","Ilość","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Ilość","","","tCO2Eq","","19.4"]
["Połączenia instalacji rurowej","Ciecz","","Śr. zewn.","mm","","12.70"]
["","Gaz","","Śr. zewn.","mm","","22.2"]
["Połączenia instalacji","Długość instalacji rurowej","Maks.","OU - IU","m","","100"]
["Podłączenie instalacji rurowej","Długość instalacji rurowej","System","Podłączenie instalacji rurowej-=-Długość instalacji rurowej-=-System-=-Bez obciążenia-=-m","m","","30"]
["Standardowe akcesoria","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Zasilanie","Częstotliwość","","","Hz","","50"]
["Prąd - 50 Hz","Maksymalne amperaże bezpiecznika (MFA)","","","A","","25"]