{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLPIR"]
[]
[]
[]
[]
["","","","","WLPIR."]
["Maks. liczba możliwych do podłączenia jedn. wewnętrznych","","","","0"]
["Maks. liczba możliwych do podłączenia jedn. zewnętrznych @","","","","0"]
["Obudowa","Kolor","","","Biały"]
["","Osłona przycisku","","","Nie"]
["","LED operacyjne","Kolor","","Zielony"]
["Wymiary","Jednostka","Wysokość","mm","113"]
["","","Szerokość","mm","72.0"]
["","","Głębokość","mm","46.0"]
["","Jednostka zapakowana","Wysokość","mm","500"]
["","","Szerokość","mm","445"]
["","","Głębokość","mm","260"]
["Ciężar","Jednostka","","kg","0.077"]
["Opakowanie","Materiał","","","Tektura"]
["","Ciężar","","kg","0.018"]
["Temp. otoczenia","Działanie","Min.","°C","0"]
["","","Maks.","°C","45"]
["","Przechowywanie","Min.","°C","0"]
["","","Maks.","°C","45"]
["","Temp. otoczenia-=-Wilgotność względna <-=-%","","%","85"]
["Instalacja","","","","Instalacja w pomieszczeniu"]