{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKMBPP1"]
[]
[]
[]
[]
["","","","","EKMBPP1."]
["Wymiary","Jednostka","Wysokość","mm","20"]
["","","Szerokość","mm","100"]
["","","Głębokość","mm","100"]
["Temperatura otoczenia","Działanie","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Przechowywanie","Min.","°C","-25"]
["","","Maks.","°C","70"]
["","Wilgotność względna <","","%","95"]
["Power supply","liczba faz","","","1~"]
["","Częstotliwość","","Hz","50/60"]
["","Napięcie","","V","15V-24V DC"]
["Złącza przewodów","Długość okablowania","Maks.","m","10"]