{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":17,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWWS-DZXE"]
[]
[]
[]
[]
["","","","","EWWS340DZXEA1","EWWS470DZXEA1","EWWS570DZXEA1","EWWS670DZXEA2","EWWS680DZXEA2","EWWS740DZXEA1","EWWS950DZXEA2","EWWSC10DZXEA3","EWWSC11DZXEA2","EWWSC14DZXEA3","EWWSC15DZXEA2","EWWSC17DZXEA3","EWWSC22DZXEA3"]
["Wydajność chłodnicza","Nom.","","kW","336.7","471.2","558","670.9","674.5","728.7","941.7","1025","1117","1420","1451","1653","2129"]
["Regulacja wydajności","Metoda","","","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna","Zmienna"]
["Regulator wydajności","Minimalna wydajność","","%","29","20","20","15","15","17","10","10","10","7","9","7","6"]
["Pobór mocy","Chłodzenie","Nom.","kW","70.2","95.1","108","140","139","130","188","210","216","287","259","324","386"]
["EER","","","","4.8","4.96","5.15","4.8","4.85","5.61","5.01","4.89","5.18","4.94","5.6","5.1","5.52"]
["ESEER","","","","0","0","0","0","0","0","0","0","0","0","0","0","0"]
["Wymiary","Jednostka","Głębokość","mm","3625","3625","3625","3625","3585","3585","3585","4688","3580","4793","3580","4768","4812"]
["","","Wysokość","mm","1865","1865","1865","1985","1985","1985","1985","2082","2200","2083","2200","2225","2290"]
["","","Szerokość","mm","1055","1055","1055","1160","1160","1160","1160","1510","1270","1510","1270","1510","1510"]
["Ciężar","Jednostka","","kg","1750","1950","2050","2850","2850","2650","3000","4400","3700","4700","3900","5100","5900"]
["","Ciężar operacyjny","","kg","2033","2276","2407","3197","3354","3162","3568","4970","4412","5370","4699","5890","6920"]
["Wodny wymiennik ciepła - parownik","Typ","","","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura"]
["","Objętość wody","","l","70","96","107","107","134","134","156","207","199","272","229","317","444"]
["Wodny wymiennik ciepła - skraplacz","Typ","","","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura","Zalana obudowa i rura"]
["Sprężarka","Typ","","","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa","Sprężarka odśrodkowa, bezolejowa"]
["","Ilość","","","1","1","1","2","2","1","2","3","2","3","2","3","3"]
["Poziom mocy akustycznej","Chłodzenie","Nom.","dBA","88","89","90","91","91","91","92","93","93","94","94","95","96"]
["Poziom ciśnienia akustycznego","Chłodzenie","Nom.","dBA","70","71","72","73","73","73","74","73","75","74","76","75","76"]
["Czynnik chłodniczy","Typ","","","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A","R-513A"]
["","Ilość","","kg","160","130","130","200","200","190","200","270","250","270","250","300","355"]
["","Obwody","Ilość","","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","GWP","","","629.5","629.5","629.5","629.5","629.5","629.5","629.5","629.5","629.5","629.5","629.5","629.5","629.5"]