{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B"]
[]
[]
[]
[]
["","","","","","FDQ125B8V3B9","FDQ200B8V3B9","FDQ250B8V3B9"]
["Wydajność chłodnicza","Całkowita wydajność","","Nom.","kW","","20.0","24.1"]
["Wydajność grzewcza","Wydajność całkowita","","Nom.","kW","","23.0","26.4"]
["Obudowa","Kolor","","","","Nie powlekana","Nie powlekana","Nie powlekana"]
["","Materiał","","","","Stal galwanizowana","Stal galwanizowana","Stal galwanizowana"]
["Wymiary","Jednostka","","Wysokość","mm","350","450","450"]
["","","","Szerokość","mm","1,400","1,400","1,400"]
["","","","Głębokość","mm","662","900","900"]
["Ciężar","Jednostka","","","kg","59.0","89.0","94.0"]
["Wymagana przestrzeń międzystropowa >","mm","","","","350","450","450"]
["Wentylator","Przepływ powietrza","Chłodzenie","Nom.","m³/min","43.0"]
["","","","Medium","m³/min","","69.0","89.0"]
["","","Grzanie","Nom.","m³/min","43.0"]
["","","","Medium","m³/min","","69.0","89.0"]
["","Spręż dyspozycyjny","","Wysoki","Pa","150","250","250"]
["","","","Nom.","Pa","150","250","250"]
["","","","Niski","Pa","150","250","250"]
["Sound power level","Chłodzenie","","","dBA","75.0","81.0","82.0"]
["Poziom ciśnienia akustycznego","Chłodzenie","","Wysoki","dBA","44.0","45.0","47.0"]
["","Grzanie","","Niski","dBA","44.0","45.0","47.0"]
["Połączenia instalacji","Ciecz","","Śr. zewn.","mm","9.52","9.52","12.70"]
["","Gaz","","Śr. zewn.","mm","15.9","22.2","22.2"]
["","Spust","","","","","OD Ø25.0","OD Ø25.0"]
["Syst. kontroli","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Standardowe akcesoria","Instrukcja obsługi i instalacji","","","","1","1","1"]
["Power supply","Nazwa","","","","V3","V3","V3"]
["","liczba faz","","","","1~","1~","1~"]
["","Częstotliwość","","","Hz","50","50","50"]
["","Napięcie","","","V","230","230 +/-10%","230 +/-10%"]
["Uwagi","","","","","(1) - Wartości dźwięku zostały zmierzone w pół-bezpogłosowym pomieszczeniu z korektami.","(1) - Wartości dźwięku zostały zmierzone w pół-bezpogłosowym pomieszczeniu z korektami.","(1) - Wartości dźwięku zostały zmierzone w pół-bezpogłosowym pomieszczeniu z korektami."]
["","","","","","(2) - Poziom ciśnienia akustycznego jest mierzony za pomocą mikrofonu z odległości 1 m od jednostki.","(2) - Poziom ciśnienia akustycznego jest mierzony za pomocą mikrofonu z odległości 1 m od jednostki.","(2) - Poziom ciśnienia akustycznego jest mierzony za pomocą mikrofonu z odległości 1 m od jednostki."]
["","","","","","(3) - Poziom ciśnienia akustycznego to wartość względna, która zależy od odległości i warunków akustycznych. W celu uzyskania informacji dodatkowych, patrz rysunki poziomu natężenia dźwięku.","(3) - Poziom ciśnienia akustycznego to wartość względna, która zależy od odległości i warunków akustycznych. W celu uzyskania informacji dodatkowych, patrz rysunki poziomu natężenia dźwięku.","(3) - Poziom ciśnienia akustycznego to wartość względna, która zależy od odległości i warunków akustycznych. W celu uzyskania informacji dodatkowych, patrz rysunki poziomu natężenia dźwięku."]
["","","","","","(4) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(4) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku.","(4) - Poziom mocy akustycznej to warto absolutna oznaczająca moc wytwarzaną przez źródło dźwięku."]
["","","","","","(5) - W celu uzyskania dodatkowych informacji, patrz schemat instalacji elektrycznej, tabliczka znamionowa i instrukcja instalacji.","(5) - W celu uzyskania dodatkowych informacji, patrz schemat instalacji elektrycznej, tabliczka znamionowa i instrukcja instalacji.","(5) - W celu uzyskania dodatkowych informacji, patrz schemat instalacji elektrycznej, tabliczka znamionowa i instrukcja instalacji."]