{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Poziom ciś. akust.","Grzanie","Wysoki","dBA","38"]
["","","Czynnik","dBA","36"]
["","","Niski","dBA","30"]
["","Chłodzenie","Medium","dBA","36"]
["","","Niski","dBA","30"]
["","","Wysoki","dBA","38"]
["Standardowe akcesoria","Instrukcja instalacji","","","1"]
["","Instrukcja obsługi","","","1"]
["","Izolacja mocowania","","","1"]
["","Podkładka uszczelniająca","","","1"]
["","Zacisk metalowy","","","1"]
["","Przewód spustowy","","","1"]
["","Podkładka do wspornika wieszaka","","","8"]
["","Materiał uszczelniający","","","2"]
["","Zaciski","","","6"]
["","Płyta mocująca z podkładką","","","4"]
["","Śruby dla kołnierzy przewodów","","","1"]
["","Filtr powietrza","","","1"]
["Piping connections","Ciecz","Śr. zewn.","mm","6.35"]
["","Gaz","Śr. zewn.","mm","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Chłodzenie","Nom.","kW","0.060"]
["","Grzanie","Nom.","kW","0.060"]
["Poziom mocy akustycznej","Chłodzenie","","dBA","55"]
["","Ogrzewanie","","dBA","55"]
["Wymiary","Jednostka","Szerokość","mm","1,150"]
["","","Głębokość","mm","620"]
["","","Wysokość","mm","200"]
["Ciężar","Jednostka","","kg","30.0"]
["Wentylator","Spręż dyspozycyjny","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Częstotliwość","","Hz","50/60"]
["","Nazwa","","","VE"]
["","Napięcie","","V","220-240"]
["Uwagi","","","","(1) - Po podłączeniu do jednostki zewnętrznej w systemie multi, patrz specyfikacje podłączanej jednostki zewnętrznej multi."]