{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLTRH"]
[]
[]
[]
[]
["","","","","WLTRH."]
["Maks. liczba możliwych do podłączenia jedn. wewnętrznych","","","","0"]
["Maks. liczba możliwych do podłączenia jedn. zewnętrznych @","","","","0"]
["Obudowa","Kolor","","","Biały"]
["","Osłona przycisku","","","Nie"]
["","LED operacyjne","Kolor","","Zielony"]
["Wymiary","Jednostka","Wysokość","mm","75"]
["","","Szerokość","mm","60.0"]
["","","Głębokość","mm","25.0"]
["","Jednostka zapakowana","Wysokość","mm","380"]
["","","Szerokość","mm","305"]
["","","Głębokość","mm","195"]
["Ciężar","Jednostka","","kg","0.036"]
["Opakowanie","Materiał","","","Tektura"]
["","Ciężar","","kg","0.0084"]
["Temp. otoczenia","Działanie","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Przechowywanie","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Temp. otoczenia-=-Wilgotność względna <-=-%","","%","100"]
["Instalacja","","","","Instalacja w pomieszczeniu"]